10 15 20 25 30 35

2300

2350

2400

2450

2500

2550

2600

Pause Time (in seconds)

Aggregate Energy Depletion (in joules) during transmission and receiving

Energy Depletion for network size = 200 nodes